|  |
| --- |
| **TOILET CUBICLE UNIT TYPE SVF30** |
|  | **The text modules shown below in blue are options that can be selected by the contracting authority as an alternative to the text printed in black. In this case, the corresponding black text must be deleted and the description “as an alternative“ removed.** |
| **MODEL:** | **TYPE SVF30** fromSchäferTrennwandsysteme GmbH, 56593 Horhausen, Phone: 02687/91510, [www.schaefer-tws.de](http://www.schaefer-tws.de) or technical and visual absolutely equal. |
| **CERTIFICATIONS, STANDARDS:** | The system is TÜV tested (German Association for Technical Inspection) and has a GS mark. The corresponding certificate must be presented. Systems without a valid TÜV GS test are not permitted.To prove the sustainability of the product, the cubicle system must be PEFC (PEFC/04-31-3143) or FSC® (FSC-C147242) certified. The corresponding certificate from the cubicles manufacturer must be presented. Systems without valid PEFC or FSC® certification are not permitted. It is not enough to provide a general certification of the used panels. The material used comply in detail with the following standards and regulations: * Chipboard panels E05 according to DIN EN 717-1
* Stainless steel according to DIN EN 10088, material quality 1.4301, respectively ASTM A276, AISI 304.
* Aluminium profiles according to DIN EN 573 and DIN EN 755, material quality EN WA6063. Surface treated (non-surface treated aluminium parts are not permitted) colourless anodized according to EURAS E6/C-0 respectively DIN 17611 E6/EV1 or powder coating according to DIN EN 12206-1.
* Adhesives and sealants may only be used if they are not subject to classification according to the EU Chemicals Regulation (CLP regulation).
* The product complies with the European regulation of registration, evaluation, approval and restriction of chemical substances (REACH). A corresponding declaration of conformity from the manufacturer can be submitted.
* Fastening materials such as screws, rivets, etc. galvanized or made of stainless steel.
 |
| **DESIGN:** | Melamine-resin coated chipboard with ABS-strips in connection with natural anodized or powder coated aluminium profiles. |
| **CONSTRUCTION:** | The outside of the cubicle has an absolute flush-fitting construction. 30 mm thick, melamine-resin chipboard panels, bonding V 20. All visible edges are coated with coloured ABS-strips, edges slightly rounded. Melamine edges are not permitted. Wall- and partition wall connections are by means of aluminium-U-profiles over the complete height of elements. An enclosing aluminium headrail, 47 x 27 mm, edges slightly rounded, runs along the top of the front panel to lend stability to the system. Front wall panels are minimum 10 mm inside of the aluminium profile. Salient profiles are not permitted. In the area along the door protective insert made of aluminium. **As an alternative:** Flame-resistant construction by the use of chipboard panels with fire protection according to Euroclass B-s2,d0 EN 13501-1. The corresponding classification certificates must be submitted. **As an alternative(not possible with cut outs in the wall connections):** wall connections are made with U-profiles as shadow gaps. |
| **DOORS:** | The construction of doors corresponds to the front wall. Butt closing doors, with a milled rebate profile made of aluminium. Therefore the outside of the cubicle has an absolute flush-fitting construction, the door opening doesn’t matter. Rebate profile made of aluminium with integrated rubber sealing for long-term noise reduction. Dampings with glazing tape are not permitted. To cover the crack of the door a coloured plastic strip is milled in on hinge side. Non-milled sight protection solutions are not permitted. |
| **HARDWARE:** | Two maintenance-free stainless steel hinges with high-performance polymer running tread. Hinges are flush milled into the ABS strips. Screwed-on hinges are not permitted. Hinges without high-performance polymer running tread are not permitted. Hinges have to pass an endurance test of 300.000 cycles without abrasion.Fully galvanised lock with latch and bolt. U-shaped safety handle of unbreakable nylon with steel core, thickness 23 mm. Rosettes, olive latch, free-/occupied-indicator und emergency unlocking device outside.**As an alternative:** Two maintenance-free stainless steel hinges made of high-performance polymers with self-closing function. That ensures a steady closing speed. Self-closing hinges as feather hinges are not permitted. Hinges have to pass an endurance test of 300.000 cycles without abrasion.**As an alternative:** Non-visible in the door rebate embedded hinges, e.g. Simonswerk Tectus without self-closing function. **As an alternative:** Non-visible in the door rebate embedded hinges, e.g. Simonswerk Tectus. Self-closing function of the doors due to a in the front not visible door closer.**As an alternative:** Fully galvanised bolt lock with stainless steel front plate. Schäfer SLIDESAFE sliding single-handed fitting made of anodised aluminium. Outside with clearly visible viewing window of at least 5 cm² for free/occupied indication and emergency release opening for hexagonal pin key. Inside, smooth-running push handle for locking and opening the door with two clearly visible viewing windows of at least 10 cm² viewing windows for the free/occupied indicator. The locking status must also be displayed inside the cabin. Fitting solutions that do not display the locking status in the cabin are not permitted. **As an alternative:** Fully galvanised lock with latch and bolt. L-shaped safety handle made of natural anodised aluminium (model Frankfurt). Rosettes, olive latch, free-/occupied-indicator and emergency unlocking device outside. Hooks and buffer also made of natural anodized aluminium.**As an alternative:** Fully galvanised lock with latch and bolt. L-shaped safety handle made of stainless steel (model Frankfurt). Rosettes, olive latch, free-/occupied indicator and emergency unlocking device outside. Hooks and buffer also made of stainless steel.**As an alternative:**Handrail on the outside of the door made of anodised aluminium, 55 x 20 mm. Length optionally 500 mm, 1.150 mm or adapted to the upper edge of the door leaf. Integrated free occupied indicator (red-white) and emergency unlocking by means of hexagon socket. On the inside with the Schäfer INSAFE one-hand door knob made of anodised aluminium with particularly easy-grip knob and two clearly visible, at least 25 mm wide viewing windows of the free/occupied indicator. The locking status must also be visible at the inside of the cubicle. Fitting solutions that do not indicate the locking status inside the cubicle are not permitted. Bolt lock with zinc die-cast bolt and stainless steel forend. **As an alternative:**In addition to the fitting specified above, free-occupied indication by means of LED display, 500 mm long, recessed in the side panel next to the door with plexiglass cover. The LED display permanently indicates the locking status of the cubicle (free = green, occupied = red). Power supply on site by means of 12 Volt DC supply line. Cable routing concealed within the partition wall elements. |
| **FEET:** | Fully height-adjustable support feet with welded-on base and flat cover plate completely made of stainless steel. Plastic feet or plastic rosettes are not permitted.**As an alternative:** Fully height-adjustable support feet with welded-on base and flat cover plate completely made of aluminium, natural anodized (E6/EV1). Plastic feet or plastic rosettes are not permitted. |
| **STANDARD ACCESSORIES:** | Per cubicles 1 hook, 1 door buffer, the material of the accessories corresponds to that of the door handles.**Optional accessories:**Schäfer hook stainless steel ES6010Schäfer hook with buffer stainless steel ES6007Schäfer toilet roll holder stainless steel ES6001Schäfer spare toilet roll holder stainless steel ES6002Schäfer toilet brush stainless steel ES6003Schäfer hook aluminium AL7010Schäfer hook with buffer aluminium AL7007Schäfer toilet roll holder aluminium AL7001Schäfer spare toilet roll holder aluminium AL7002Schäfer toilet brush aluminium AL7003 |
| **COLOURS:** | Panels and hardware according to manufacturer’s colour chart. Profiles plastic coated (powder coating) according to colour chart or natural anodized (E6/EV1).**As an alternative:**BLACKLINE variant: Design variant in black. Schäfer INSAFE one-hand door knob or lever handle set and all other door fittings (hinges, hooks, buffers) made of black anodised aluminium. |
| **HEIGHT:** | Standard height 2.000 mm incl. 150 mm clearance.**As an alternative:** height 2.150 mm incl. 150 mm clearance. |
| **ACCESSORIES:****09/2024** | Privacy screen 400 x 900 mm, made of the same material as the cubicle elements, wall mounted. Fastening by two anodized aluminium brackets, which are screwed invisibly onto the back of the privacy screen and additionally stabilise it. Aluminium brackets with contact surface to the brick wall, which is additionally provided with adhesive, to give a maximum hold.**As an alternative:** Privacy screen 400 x 900 mm, made of 10 mm thick safety glass with ceramic screen printing on one side. Wall mounted with four anodized aluminium brackets. |