|  |  |
| --- | --- |
| WC **KIDDIES** PRIVACY SCREEN TYPE VK13 KIGA | |
|  | The text modules shown in blue below are options that can be selected by the tendering body as an alternative to the text printed in black. In this case, the corresponding black text must be deleted and the designation "As alternative" removed. |
| **FABRICATE:** | **TYPE KIDDIES PRIVACY SCREEN VK13** KIGA from Schäfer  Trennwandsysteme GmbH, 56593 Horhausen, Tel. 02687/91510, [www.schaefer-tws.de](http://www.schaefer-tws.de/) or technically and visually absolutely equivalent. |
| **CERTIFICATIONS, STANDARDS:** | The system is TÜV tested and has the GS mark. The corresponding certificate must be presented. Systems without a valid TÜV GS test are not approved.  To prove the sustainability of the product, the cubicle system must be PEFC (PEFC/04-31-3143) or FSC® (FSC-C147242) certified. The corresponding certificate of the system manufacturer must be presented. Systems without valid PEFC or FSC® certification are not permitted. It is not sufficient to present a general certificate of the panels used.  The materials used comply with the following standards and regulations:   * HPL compact panels according to DIN EN 438-7 * Stainless steel according to DIN EN 10088, material grade 1.4301, or ASTM A276, AISI 304 * Extruded aluminium profiles according to DIN EN 573 and DIN EN 755, material grade EN WA6063. Surface-treated (non-surface-treated aluminium parts are not permitted) colourless anodised according to EURAS E6/C-0 or DIN 17611 E6/EV1 or powder coating according to DIN EN 12206-1. * Adhesives and sealants may only be used if they are not subject to classification according to the EU Chemicals Regulation (CLP Regulation). * The product is compliant with the European Regulation on Registration, Evaluation, Authorisation and Restriction of Chemicals (REACH). A corresponding declaration of conformity from the manufacturer can be provided. * Fasteners, such as screws, rivets, etc. galvanised or made of stainless steel |
| **DESIGN**: | Waterproofed HPL solid core panels, in combination with colour- coated, vertical and horizontal aluminium profiles. Absolutely water-resistant, rot-proof, scratch-, break- and impact-resistant. |
| **CONSTRUCTION:** | Kiddies privacy screen for mounting between children's WC pots as a simple privacy screen. Dimensions approx. 850 mm x 900 mm (height x depth). All corners and edges have a minimum radius  of 5 mm in accordance with GUV guidelines. |
| **DECLARATIONS:** | Fastening to the rear wall by means of aluminium U-profile, closed head. Front support by means of anodised aluminium base, rounded for body comfort, fixing screws concealed under aluminium cover rosette. |
| **COLOURS:**  **05/2022** | Panels and fittings according to manufacturer´s colour chart. Profiles and fittings natural anodized (E6/EV1). |